Model GC5 – 0 degree deflection

The return grilles shall be model GC5 by Anemostat and shall integrate with the ceiling style as scheduled. The core shall be an aluminum grid consisting of a 1/2" x 1/2" x 1/2" cells, and shall have a minimum free area of 90%.  For surface mounting applications, the border shall be extruded aluminum, and shall include countersunk screw holes for installation. Lay-in models shall include extension panels where required for the scheduled duct size and grid system module size.  The grilles shall have a baked-on arctic white finish.

Provide optional steel or aluminum opposed blade volume control dampers as scheduled. Dampers shall be adjustable through the face of the register.
---------------------------------------------------------------------------------------------------------------------
Model GC5NS – No-Site 45 degree deflection

The return grilles shall be model GC5NS by Anemostat and shall integrate with the ceiling style as scheduled. The core shall be an aluminum grid consisting of a 1/2" x 1/2" x 1/2" cells, with 45 degree deflection angle.  For surface mounting applications, the border shall be extruded aluminum, and shall include countersunk screw holes for installation. Lay-in models shall include extension panels where required for the scheduled duct size and grid system module size.  The grilles shall have a baked-on arctic white finish.

Provide optional steel or aluminum opposed blade volume control dampers as scheduled. Dampers shall be adjustable through the face of the register.