HD35-MS - Medium Security With Fixed 0° or 40° louver

Contractor shall furnish and install security grilles, type HD35-MS, as herein specified or where shown on plans. The units shall be as manufactured by Anemostat Products. Security grille type HD35-MS shall be all steel welded construction. Louver bars are constructed of 13 GA round edge steel spaced 1/2" on center. The louver bars will have either zero of 40 degree deflection, as required to meet job conditions. The frame shall be 16 GA C.R.S. with welded corners. The support bars shall be 13 GA round edge steel welded to the frame, with a maximum spacing (center to center) of 6 inches. The interior screen consists of 
10 GA x 1/2" woven steel mesh on 5/8" centers. The heavy gauge screen is welded to the frame. The unit shall be installed with tamperproof screws. The HD35-MS unit shall be finished with factory white powder coat finish.