ASSG - Maximum Security GRille with Steel Perforated Face

Contractor shall furnish and install the security grille, type ASSG, as herein specified or where shown on plans. The unit shall be as manufactured by Anemostat Products. Security grille type ASSG shall be all steel welded construction. Sleeve shall be 12 GA C.R.S. with continuous welds to the face plate. The face plate shall be 3/16" C.R.S. with a perforated pattern of 1/4" diameter holes on 3/8" staggered centers. The locking angles shall be shipped loose for field welding by others to the sleeve. The ASSG shall be finished with factory white powder coat finish. Note: round sleeve shall be 12 GA.