Model SAG - Stamped Architectural Grilles & Registers
 
Contractor shall furnish and install stamped architectural grilles/registers, Model SAG, as herein specified or where shown on plans. The unit shall be as manufactured by Anemostat Products. The stamped grille shall be fabricated from (Steel) (Aluminum) (304 Stainless Steel) (Brass) (Bronze) and shall be perforated with Anemostat Pattern (insert pattern Pxx).  Material thickness shall be  (insert thickness/gauge). #8 screws shall be provided by the manufacturer for attaching the face plate to a suitable edge. Finish shall be (Arctic White Powder Coat) (Painted Color) (#4 Satin Polish) (#8 Mirror) (Custom matched color) (Satin Anodize).